3.1a) Given that the input frequency F\_0 is 15 Hz, the sampling frequency must be 2 \* the F\_Max of the input signal. Thus the sampling frequency F\_s must be at least 30 Hz

3.1b)